# Dell Memory Upgrade - 32GB - 2RX8 DDR4 UDIMM 3200MHz ECC

Dell Part AB806062

Random Access Memory (RAM) is a type of hardware that your computer uses to store information. Adding memory is one of the most cost-effective ways to improve your computer's performance.

## Media

### Why should I buy a Dell Upgrades over a third-party part?

### Tested and Verified Tier-1 OEM-Grade Parts

Ensure compatibility with Dell servers, storage and networking.

### Ease of Installation

Save time with Dell Upgrades that are shipped as kits with the necessary hardware and firmware.

### Secure Supply Chain Focus

Protect system data and integrity with parts sourced from a secure supply chain.

### Dell Tech Support and Warranties

Preserve Dell technical support and warranties—which do not support systems with third-party upgrades.

### Compatibility

This product is compatible with the following systems:

- PowerEdge R250
- PowerEdge R350
- PowerEdge T150
- PowerEdge T350
- Precision Workstation 3450 SFF
- Precision Workstation 3450XE SFF
- Precision Workstation 3640 Tower
- Precision Workstation 3640XE Tower
- Precision Workstation 3650 Tower
- Precision Workstation 3650XE Tower
- Precision Workstation R3930
- Precision Workstation R3930 XL

### Memory DIMM Types

### With more memory, the faster that data and instructions can be read, written, and performed by the server.

There are three types of memory DIMMS for servers available. These DIMM types cannot be mixed in a single system, you must select the type of DIMM appropriate for your workload at the type of purchase.

- Unbuffered DIMM: UDIMM, an unbuffered, low density, low-latency DIMM that doesn't include a register or buffer chip. UDIMMs are generally used in applications requiring the lowest possible latency.
- Registered DIMM: RDIMM, a registered DIMM that provides high signal integrity -- performing parity checking to detect improper addresses or commands -- and increased performance for heavy workloads.
- Load reduced DIMMs: LRDIMM, uses a buffer to reduce memory loading to a single load on all DDR signals, allowing for greater density

### Memory Tests

- Burn-in: Powered stress testing (i.e. increased temperature) to remove weak components.
- Component Test: Memory vendor-specific diagnostic tests performed at DRAM component level to ensure functionality.
- Module Test: Memory vendor-specific diagnostic tests performed at DIMM level to ensure functionality (with all DRAM components already mounted on DIMM PCB).