
2025.06.12 V1.14
1. Fix the problem that the APRS beacon list cannot be entered
2. "PTT After" adds "Area Match" and "All Area" options. If "Area Match" is set, the PTT beacon will only transmit the ARPS beacon on the channel when the transmission channel is the same as the channel set by "PTT After CH". If "All Area" is set, the APRS beacon will be sent one by one from the channel set by "PTT After CH" at the end of each transmission.